Product Information

# Command Lists

> EPSON ESC/P 2 control codes
> IBM 2390 Plus emulation control codes

Your printer supports the EPSON ESC/P 2 control codes and IBM 2390 Plus emulation control codes listed below.

## EPSON ESC/P 2 control codes

Selecting an EPSON ESC/P 2 printer in your software allows you to use advanced fonts and graphics.

General operation:
| ESC @, ESC U, ESC EM
Paper feeding:
| FF, LF, ESC 0, ESC 2, ESC 3, ESC +, CR
Page format:
| ESC (C, ESC C, ESC C 0, ESC Q, ESC l, ESC (c, ESC N, ESC O
Print position motion:
| ESC $, ESC \, ESC (V, ESC (v, ESC D, HT, ESC B, VT, ESC J
Font selection:
| ESC k, ESC x, ESC y, ESC X, ESC P, ESC M, ESC g, ESC p, ESC 4, ESC 5, ESC E, ESC F, ESC !
Font enhancement:
| ESC W, DC4, SO, DC2, SI, ESC w, ESC G, ESC H, ESC T, ESC S, ESC -, ESC (-, ESC q
Spacing:
| ESC Space, ESC c, ESC (U
Character handling:
| ESC t, ESC (t, ESC R, ESC %, ESC &, ESC :, ESC 6, ESC 7, ESC (^
Bit image:
| ESC *
Bar code:
| ESC (B
Color printing:
| ESC r

[Top]

## IBM 2390 Plus emulation control codes

This printer emulates the IBM Proprinter using the commands below. For detailed information, see the IBM 2390 Plus reference manual.

General operation:
| NUL, DC3, ESC j, BEL, CAN, DC1, ESC Q, ESC [ K, ESC U, ESC [ F
Paper feeding:
| FF, LF, ESC 5, ESC A, ESC A (AGM*), ESC 0, ESC 1, ESC 2, ESC 3, ESC 3 (AGM*), CR, ESC ]
Page format:
| ESC C, ESC C0, ESC X, ESC N, ESC O, ESC 4
Print position motion:
| ESC d, ESC R, ESC D, HT, ESC B, VT, ESC J, ESC J (AGM*)
Font selection:
| DC2, ESC P, ESC :, ESC E, ESC F, ESC I, ESC [d, ESC [I
Font enhancement:
| DC4, SO, ESC SO, ESC W, ESC [ @, SI, ESC SI, ESC G, ESC H, ESC T, ESC S, ESC -, ESC _, ESC [-
Spacing:
| BS, SP, ESC [\
Character handling:
| ESC 6, ESC 7, ESC [T, ESC ^, ESC \
Bit image:
| ESC K, ESC L, ESC Y, ESC Z, ESC [g, ESC*(AGM*)
Bar code:
| ESC [f, ESC [p
Download:
| Download Command is not provided.

* Alternate Graphic Mode

[Top]

Previous | Next