# Index

#

0 slash,

- About Your Printer's Default Settings

A.G.M. (Alternate Graphic Mode),

- About Your Printer's Default Settings

Adjusting

> paper thickness lever,
> - Adjusting the paper thickness lever

> tear-off position,
> - Adjusting the tear-off position

> top-of-form position,
> - Adjusting the top-of-form position

Aligning vertical lines,

- Printing a Self Test

Auto CR (carriage return),

- About Your Printer's Default Settings

Auto I/F (interface) wait time,

- About Your Printer's Default Settings

Auto line feed,

- About Your Printer's Default Settings

Auto tear-off,

- About Your Printer's Default Settings

Baud rate,

- About Your Printer's Default Settings

Bidirectional (Bi-d) printing.,

- About Your Printer's Default Settings

Built-in font

> list,
> - Electronic

Buttons.,

- Using the Control Panel

Buzzer (beeper) setting,

- About Your Printer's Default Settings

Canceling printing,

- Canceling Printing

Character table

> list,
> - Electronic

> setting,
> - About Your Printer's Default Settings

Cleaning the printer,

- Cleaning the Printer

Clients

> with Windows Me or 98,
> - With Windows Me or 98

> with Windows NT 4.0,
> - With Windows NT 4.0

> with Windows XP or 2000,
> - With Windows XP or 2000

Contacting EPSON,

- Before Contacting Epson

Continuous paper

> printing,
> - Printing on Continuous Paper

> specifications,
> - Paper

Control panel,

- Using the Control Panel

- Using the Error Indicators

Customer support,

- Before Contacting Epson

Cut-sheet feeder,

- Cut-sheet feeder

Data length,

- About Your Printer's Default Settings

Default settings

> changing,
> - Changing default settings

> option list,
> - About Your Printer's Default Settings

Driver (printer driver),

- About Your Printer Software

Emulation.,

- IBM 2390 Plus emulation control codes

Envelopes

> printing,
> - Envelopes

> specifications,
> - Paper

EPSON Status Monitor 3,

- About Your Printer Software

- Using EPSON Status Monitor 3

> accessing,
> - Accessing EPSON Status Monitor 3

> installing,
> - Installing EPSON Status Monitor 3

> setting up,
> - Setting up EPSON Status Monitor 3

Error indication,

- Using the Error Indicators

ESC/P 2,

- EPSON ESC/P 2 control codes

Font,

- About Your Printer's Default Settings

Font (default setting),

- About Your Printer's Default Settings

High speed draft (default setting),

- About Your Printer's Default Settings

I/F (interface) mode,

- About Your Printer's Default Settings

IBM 2390 Plus emulation,

- IBM 2390 Plus emulation control codes

International character set for Italic table,

- About Your Printer's Default Settings

International character sets,

- Electronic

Labels

> printing,
> - Labels

> specifications,
> - Paper

Lights.,

- Using the Control Panel

Manual feed wait time,

- About Your Printer's Default Settings

Micro adjust,

- Adjusting the top-of-form position

- Adjusting the tear-off position

Multipart forms

> printing,
> - Multipart forms

> specifications,
> - Paper

Options

> Color upgrade kit,
> - Color upgrade kit

> Cut-sheet feeder,
> - Cut-sheet feeder

> Pull tractor unit,
> - Pull tractor unit

> Roll paper holder,
> - Roll paper holder

Packet mode,

- About Your Printer's Default Settings

Page length for tractor,

- About Your Printer's Default Settings

Panel.,

- Using the Control Panel

Paper alignment,

- Paper alignment

Paper specifications,

- Paper

Paper thickness lever,

- Adjusting the paper thickness lever

Parallel I/F (interface) bidirectional mode,

- About Your Printer's Default Settings

Parity,

- About Your Printer's Default Settings

Pitch,

- About Your Printer's Default Settings

Printable area,

- Printable area

Print direction,

- About Your Printer's Default Settings

Printer

> sharing,
> - Sharing the printer

Printer driver

> accessing

> > from Windows Me or 98,
> > - Accessing the printer driver from Windows applications

> > from Windows XP, 2000 or Windows NT 4.0,
> > - Accessing the printer driver from Windows applications

> settings,
> - Printer Driver Settings Overview

> uninstalling,
> - Uninstalling the Printer Software

Removing

> printed document from

> > push tractor,
> > - Removing a printed document from the push tractor

Ribbon cartridge,

- Mechanical

Roll paper

> printing,
> - Roll paper holder

> specifications,
> - Paper

Roll paper holder,

- Roll paper holder

Self test,

- Printing a Self Test

Single sheets

> printing,
> - Printing on Single Sheets

> specifications,
> - Paper

Skip over perforation,

- About Your Printer's Default Settings

Software

> default setting,
> - About Your Printer's Default Settings

Specifications

> built-in font,
> - Electronic

> character tables,
> - Electronic

> command lists

> > ESC/P 2,
> > - EPSON ESC/P 2 control codes

> > IBM 2390 Plus emulation,
> > - IBM 2390 Plus emulation control codes

> electrical,
> - Electrical

> environmental,
> - Environmental

> international character sets,
> - Electronic

> mechanical,
> - Mechanical

> paper,
> - Paper

> paper alignment,
> - Paper alignment

> printable area,
> - Printable area

Status Monitor 3,

- Using EPSON Status Monitor 3

Tear-off,

- Advancing the paper to the tear-off edge

> adjusting,
> - Adjusting the tear-off position

> automatically,
> - Advancing the paper to the tear-off position automatically

> button,
> - Using the Tear Off button

Technical support,

- Before Contacting Epson

Transporting the printer,

- Transporting the Printer

Troubleshooting

> USB problems,
> - Correcting USB Problems

Unidirectional (Uni-d) printing.,

- About Your Printer's Default Settings

Uninstalling

> printer software,
> - Uninstalling the Printer Software

> USB device driver,
> - Uninstalling the USB device driver

USB interface,

- About Your Printer's Default Settings

> problems,
> - Correcting USB Problems