Product Information

# Command Lists

> EPSON ESC/P control codes
> IBM 2380 Plus (for LX-300+II)/ IBM 2381 Plus (for LX-1170II) emulation control codes

Your printer supports the EPSON ESC/P control codes and IBM 2380 Plus (for LX-300+II)/IBM 2381 Plus (for LX-1170II) emulation control codes listed below.

## EPSON ESC/P control codes

Selecting an EPSON ESC/P printer in your software allows you to use advanced fonts and graphics.

General operation:
| ESC @, ESC U, ESC EM
Paper feeding:
| FF, LF, ESC 0, ESC 1, ESC 2, ESC 3, ESC A, CR
Page format:
| ESC (C, ESC C, ESC C 0, ESC Q, ESC l, ESC (c, ESC N, ESC O, ESC (U
Print position motion:
| ESC $, ESC \, ESC D, HT, ESC B, VT, ESC J
Font selection:
| ESC k, ESC x, ESC y, ESC P, ESC M, ESC g, ESC p, ESC 4, ESC 5, ESC E, ESC F, ESC !
Font enhancement:
| ESC W, DC4, SO, DC2, SI, ESC w, ESC G, ESC H, ESC T, ESC S, ESC -
Spacing:
| ESC Space
Character handling:
| ESC t, ESC (t, ESC R, ESC %, ESC &, ESC :, ESC I, ESC 6, ESC 7
Bit image:
| ESC K, ESC L, ESC Y, ESC Z, ESC *, ESC ^
Bar code:
| ESC (B
Color printing (LX-300+II only):
| ESC r

[Top]

## IBM 2380 Plus (for LX-300+II)/ IBM 2381 Plus (for LX-1170II) emulation control codes

This printer emulates the IBM Proprinter using the commands below. For detailed information, see the IBM 2380 Plus (for LX-300+II)/IBM 2381 Plus (for LX-1170II) reference manual.

General operation:
| NUL, DC3, ESC j, BEL, CAN, DC1, ESC Q, ESC [ K, ESC U, ESC [ F
Paper feeding:
| FF, LF, ESC 5, ESC A, ESC 0, ESC 1, ESC 2, ESC 3, CR, ESC ]
Page format:
| ESC C, ESC C0, ESC X, ESC N, ESC O, ESC 4
Print position motion:
| ESC d, ESC R, ESC D, HT, ESC B, VT, ESC J
Font selection:
| DC2, ESC P, ESC :, ESC E, ESC F, ESC I, ESC [d, ESC [I
Font enhancement:
| DC4, SO, ESC SO, ESC W, ESC [ @, SI, ESC SI, ESC G, ESC H, ESC T, ESC S, ESC -, ESC _
Spacing:
| BS, SP
Character handling:
| ESC 6, ESC 7, ESC [T, ESC ^, ESC \
Bit image:
| ESC K, ESC L, ESC Y, ESC Z
Bar code:
| ESC [f, ESC [p
Download:
| ESC = (only Draft mode)

[Top]

Previous | Next